Overview | Package | Class | Use | Tree | Index
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

B C D F G H L M O P R S V W X

## C

close() - Method in interface com.moxa.mxuportapi.MxUPort
  Closes the serial port.
com.moxa.mxuportapi - package com.moxa.mxuportapi
CTS - Variable in class com.moxa.mxuportapi.MxUPort.ModemStatus
  Available constants: `CTS_ON`, `CTS_OFF`.
CTS_FLOW_ENABLE - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines CTS hardware flow control
CTS_OFF - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines CTS state OFF
CTS_ON - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines CTS state ON

Overview | Package | Class | Use | Tree | Index
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

B C D F G H L M O P R S V W X