Overview | Package | Class | Use | Tree | Index
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

B C D F G H L M O P R S V W X

## R

read(byte[]) - Method in interface com.moxa.mxuportapi.MxUPort
  Reads data from the port; returns the data if the buffer is full.
read(byte[], int) - Method in interface com.moxa.mxuportapi.MxUPort
  Reads data from a port; returns the data if the given length of data has been received.
read(byte[], int, int) - Method in interface com.moxa.mxuportapi.MxUPort
  Reads data from the port; returns the data if the given length of data has been received.
requestPermission(Context, UsbManager, String, int, int, BroadcastReceiver) - Static method in class com.moxa.mxuportapi.MxUPortService
  Requests USB permission to access; should get user's permission to access the USB device.
RI - Variable in class com.moxa.mxuportapi.MxUPort.ModemStatus
  Available constants: `RI_ON`, `RI_OFF`.
RI_OFF - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines RI state OFF
RI_ON - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines RI state ON
RTS_FLOW_ENABLE - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines RTS hardware flow control
RTS_OFF - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines RTS state OFF
RTS_ON - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines RTS state ON
RtsCts - Variable in class com.moxa.mxuportapi.MxUPort.FlowCtrl
  Available ORed constants `RTS_FLOW_ENABLE`, `CTS_FLOW_ENABLE`, `RTSCTS_FLOW_ENABLE`.
RTSCTS_FLOW_ENABLE - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines RTS/CTS hardware flow control
RTSCTS_FLOW_MASK - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines bit mask of RTS/CTS hardware flow control

Overview | Package | Class | Use | Tree | Index
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

B C D F G H L M O P R S V W X