Overview | Package | Class | Use | Tree | Index
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

B C D F G H L M O P R S V W X

## D

DATA_BITS_5 - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines serial communication with 5 data bits
DATA_BITS_6 - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines serial communication with 6 data bits
DATA_BITS_7 - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines serial communication with 7 data bits
DATA_BITS_8 - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines serial communication with 8 data bits
dataBits - Variable in class com.moxa.mxuportapi.MxUPort.IoctlMode
  Available constants: `DATA_BITS_5`, `DATA_BITS_6`, `DATA_BITS_7`, `DATA_BITS_8`.
DCD - Variable in class com.moxa.mxuportapi.MxUPort.ModemStatus
  Available constants: `DCD_ON`, `DCD_OFF`.
DCD_OFF - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines DCD state OFF
DCD_ON - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines DCD state ON
DSR - Variable in class com.moxa.mxuportapi.MxUPort.ModemStatus
  Available constants: `DSR_ON`, `DSR_OFF`.
DSR_FLOW_ENABLE - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines DSR hardware flow control
DSR_OFF - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines DSR state OFF
DSR_ON - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines DSR state ON
DTR_FLOW_ENABLE - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines DTR hardware flow control
DTR_OFF - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines DTS state OFF
DTR_ON - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines DTS state ON
DtrDsr - Variable in class com.moxa.mxuportapi.MxUPort.FlowCtrl
  Available ORed constants `DTR_FLOW_ENABLE`, `DSR_FLOW_ENABLE`, `DTRDSR_FLOW_ENABLE` The default is disabled.
DTRDSR_FLOW_ENABLE - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines DTR/DSR software flow control
DTRDSR_FLOW_MASK - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines the bit mask of DTR/DSR hardware flow control

Overview | Package | Class | Use | Tree | Index
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

B C D F G H L M O P R S V W X