Overview | Package | Class | Use | Tree | Index
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

B C D F G H L M O P R S V W X

## S

setBaud(int) - Method in interface com.moxa.mxuportapi.MxUPort
  Sets the baud rate using the actual speed value.
setBreak(int) - Method in interface com.moxa.mxuportapi.MxUPort
  Sends out a break signal.
setDTR(int) - Method in interface com.moxa.mxuportapi.MxUPort
  Sets the DTR state for a serial port.
setFlowCtrl(MxUPort.FlowCtrl) - Method in interface com.moxa.mxuportapi.MxUPort
  Sets the hardware and/or software flow control.
setInterface(int) - Method in interface com.moxa.mxuportapi.MxUPort
  Sets the interface for products that support multiple interface.
setIoctlMode(MxUPort.IoctlMode) - Method in interface com.moxa.mxuportapi.MxUPort
  Configures communication parameters, such as baud rate, parity, data bits and stop bits.
setPortName(String) - Method in interface com.moxa.mxuportapi.MxUPort
  Sets the port name on the device.
setRTS(int) - Method in interface com.moxa.mxuportapi.MxUPort
  Sets the RTS state for a serial port.
setUsbReadTimeout(int) - Method in interface com.moxa.mxuportapi.MxUPort
  Sets the read timeout value for a USB read request.
setUsbWriteTimeout(int) - Method in interface com.moxa.mxuportapi.MxUPort
  Sets the write timeout value for a USB write request.
STOP_BITS_1 - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines 1 stop bit on serial communication
STOP_BITS_1_5 - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines 1.5 stop bits on serial communication
STOP_BITS_2 - Static variable in interface com.moxa.mxuportapi.MxUPort
  Defines 2 stop bits on serial communication
stopBits - Variable in class com.moxa.mxuportapi.MxUPort.IoctlMode
  Available constants: `STOP_BITS_1`, `STOP_BITS_1_5`, `STOP_BITS_2`.

Overview | Package | Class | Use | Tree | Index
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

B C D F G H L M O P R S V W X