
Product:	Moxa Smartio/Industio Windows x64 Driver
Version:	1.20
Date:		11/22/2012
Company:	Moxa Inc.

Support Platform:
-----------------
Windows XP (x64)
Windows Server 2003 (x64)
Windows Vista (x64)
Windows Server 2008 (x64)
Windows Server 2008 R2
Windows 7 (x64)
Windows 8 (x64)
Windows Server 2012

Supported Moxa Product:
------------------------
CP-102E, CP-102EL, CP-132EL, CP-132EL-I
CP-102U, CP-102UL
CP-132UL-I, CP-132UL,
CP-132, CP-132I, CP132S, CP-132IS, 
CI-132, CI-132I, CI-132IS, 
CP-102UF-S, CP-102UF-M
(C102H, C102HI, C102HIS, C102P, CP-102, CP-102S)

CP-114EL, CP-114EL-I
CP-104EL, CP-104UL, CP-104JU, CP-104EL-A
CP-134U, CP-134U-I
C104H/PCI, C104HS/PCI, 
CP-114, CP-114I, CP-114S, CP-114IS,
C104H, C104HS, 
CI-104J, CI-104JS
CI-134, CI-134I, CI-134IS, 
(C114HI, CT-114I, C104P)

CP-118EL, CP-118U, CP-118EL-A
CP-168EL, CP-168U, CP-168EL-A
C168H/PCI,  
C168H, C168HS, 
(C168P)

CB-108, CB-114, CB-134I
CP-118U-I, CP-138U, CP-138U-I
POS-104UL

CP-114UL, CP-114UL-I
CP-112UL, CP-112UL-I

Release Note:
--------------
Ver1.20 Build 12112220
1. New: Support Windows 8
2. New: Support Windows Server 2012
3. Improve: Allow to use IOCTL_SERIAL_SET_FIFO_CONTROL to clear RX FIFO
           (with value 0x02) or TX FIFO (with value 0x04.)
4. Bugfix: Flush TX FIFO more times to prevent serial port send unknown data 
           out when application close port
5. Bugfix: Fixed the bug that linear baudrate not support below 200 bps

Ver1.19 Build 11062215
1.  New: Support linear baud rate for MUE-250/450/850 UART.
2.  Improve: Prevent the malfunction of serenum driver in Windows 7 x86.
3.  Bugfix: Fixed the bug that diagnostic can't detect CP-104EL, CP-118EL,
    CP-168EL.
4.  Bugfix: Fixed the bug of S/W flow control.
5.  Bugfix: Fixed receive the same data twice when call PurgeComm() after
    ReadFile().

Ver1.18
1. Support CP-104EL-A, CP-168EL-A, CP-118EL-A.

Ver1.17
1. Support CP-114UL-I, CP-112UL, CP-112UL-I

Ver1.16 
1. Official released
2. Support CP-102E, CP-102EL, CP-132EL, CP-132EL-I, CP-114EL, CP-114EL-I

-End-
