- Main
- Tutorials
- Library
- Samples

- File List
- Globals

Namespaces | Functions | Variables
tc.py File Reference

TC Sample More...

Go to the source code of this file.

## Namespaces
| tc

## Functions
def | main ()

## Variables
int | TC_SENSOR_TYPE_K = 1

## Detailed Description

TC Sample

Copyright
  2019 Moxa Inc. All rights reserved.

Date
  2019-02-11

Author
  William Chang

Version
  V1.0
  1 '''
  2 Copyright (C) 2019 Moxa Inc. All rights reserved.
  3 SPDX-License-Identifier: Apache-2.0
  4
  5 TC Python Sample Application
  6
  7 Date Author Comment
  8 2019-02-11 William Chang Created it.
  9 '''
  10
  11
  19
  20 from ioThinx_4530 import ioThinx_4530_API
  21 import argparse
  22
  23 TC_SENSOR_TYPE_K = 1
  24
  25
  26 def main():
  27 parser = argparse.ArgumentParser(description="TC sample program.")
  28 parser.add_argument("-s", "--slot", dest="tc_slot", type=int, default=7)
  29 parser.add_argument("-c", "--channel_start", dest="tc_channel_start", type=int, default=0)
  30 parser.add_argument("-n", "--channel_count", dest="tc_channel_count", type=int, default=2)
  31 args = parser.parse_args()
  32
  33 tc_slot = args.tc_slot
  34 tc_channel_start = args.tc_channel_start
  35 tc_channel_count = args.tc_channel_count
  36 print("TC slot = {}".format(tc_slot))
  37 print("TC start channel = {}".format(tc_channel_start))
  38 print("TC channel count = {}".format(tc_channel_count))
  39
  40 # initialize ioThinx I/O
  41 device = ioThinx_4530_API.ioThinx_4530_API()
  42
  43 # temporarily set config
  44 tc_types = [TC_SENSOR_TYPE_K] * tc_channel_count
  45 device.ioThinx_TC_Config_SetSensorTypes(tc_slot, tc_channel_start, tc_channel_count, tc_types)
  46
  47 # reload config
  48 device.ioThinx_IO_Config_Reload()
  49
  50 # get value
  51 while True:
  52 tc_values = device.ioThinx_TC_GetValues(tc_slot, tc_channel_start, tc_channel_count)
  53 tc_statuss = device.ioThinx_TC_GetStatuss(tc_slot, tc_channel_start, tc_channel_count)
  54 for i in range(tc_channel_count):
  55 print("[ {}:{}] value = {}, status = {}".format(tc_slot, tc_channel_start + i, tc_values[i], tc_statuss[i]))
  56 if input("Press 'q' to exit. other keys to continue") == 'q':
  57 break
  58
  59
  60 if __name__ == '__main__':
  61 main()

Definition in file tc.py.