- Main
- Tutorials
- Library
- Samples

- File List
- Globals

pwr.py
Go to the documentation of this file.
1 '''
2 Copyright (C) 2019 Moxa Inc. All rights reserved.
3 SPDX-License-Identifier: Apache-2.0
4
5 Power Diagnostic Python Sample Application
6
7 Date Author Comment
8 2019-02-11 William Chang Created it.
9 '''
10
11
19
20 from ioThinx_4530 import ioThinx_4530_API
21 import argparse
22
23
24 def main():
25 parser = argparse.ArgumentParser(description="PWR sample program.")
26 parser.add_argument("-s", "--slot", dest="pwr_slot", type=int, default=11)
27 parser.add_argument("-a", "--alarm_voltage", dest="alarm_voltage", type=int, default=20.0)
28 args = parser.parse_args()
29
30 pwr_slot = args.pwr_slot
31 alarm_voltage = args.alarm_voltage
32 sys_channel = 0
33 field_channel = 0
34 sys_status = 0
35 field_status = 0
36 print("Power slot = {}".format(pwr_slot))
37 print("Alarm setting = {}".format(alarm_voltage))
38
39 # initialize ioThinx I/O
40 device = ioThinx_4530_API.ioThinx_4530_API()
41
42 # temporarily set config
43 device.ioThinx_PWR_Config_SetAlarms(pwr_slot, field_channel, 1, [alarm_voltage])
44
45 # reload config
46 device.ioThinx_IO_Config_Reload()
47
48 while True:
49 sys_status = device.ioThinx_PWR_GetSysStatus(pwr_slot, sys_channel, 1)
50 field_status = device.ioThinx_PWR_GetFieldStatus(pwr_slot, field_channel, 1)
51 print("[ {}] system power status = {}".format(pwr_slot, sys_status))
52 print("[ {}] filed power status = {}".format(pwr_slot, field_status))
53 if input("Press 'q' to exit. other keys to continue") == 'q':
54 break
55
56
57 if __name__ == '__main__':
58 main()
pwr.main
def main()
Definition: pwr.py:24
format
char const int const cJSON_bool format
Definition: cJSON.h:161