- Main
- Tutorials
- Library
- Samples

- Namespace List
- Namespace Members

- All
- Functions
- Variables

- AI_RANGE_4_20mA_BURNOUT : ai
- BIN_TYPE : ioThinx_4530.ioThinx_4530_API
- BUF_LEN : uart
- CNT_TRIGGER_BOTH : counter
- DI_MODE_COUNTER : counter
- DO_MODE_PWM : pwm
- LED_CHANNEL_U1 : misc
- LED_CHANNEL_U2 : misc
- LED_STATE_DARK : misc
- LED_STATE_GREEN : misc
- LED_STATE_RED : misc
- name : setup
- packages : setup
- RTD_SENSOR_TYPE_PT100 : rtd , rtd_calibration
- SLOT_CH_NUM : ioThinx_4530.ioThinx_4530_API
- TC_SENSOR_TYPE_K : tc , tc_calibration
- UART_MODE_RS232 : uart
- UART_PORT_1 : uart
- version : setup