B C D F G I L M O P R S V W X

## S

setBaud(int) - Method in interface com.moxa.mxnportapi.MxNPort
  Sets the baud rate using the actual speed value.
setBreak(int) - Method in interface com.moxa.mxnportapi.MxNPort
  Sends out a break signal.
setDTR(int) - Method in interface com.moxa.mxnportapi.MxNPort
  Sets the DTR state for a serial port.
setFlowCtrl(MxNPort.FlowCtrl) - Method in interface com.moxa.mxnportapi.MxNPort
  Sets the hardware and/or software flow control.
setIoctlMode(MxNPort.IoctlMode) - Method in interface com.moxa.mxnportapi.MxNPort
  Configure communication parameters, such as baud rate, parity, data bits, stop bits and flow control settings.
setRTS(int) - Method in interface com.moxa.mxnportapi.MxNPort
  Sets the RTS state for a serial port.
STOP_BITS_1 - Static variable in interface com.moxa.mxnportapi.MxNPort
  Defines 1 stop bit on serial communication
STOP_BITS_1_5 - Static variable in interface com.moxa.mxnportapi.MxNPort
  Defines 1.5 stop bits on serial communication
STOP_BITS_2 - Static variable in interface com.moxa.mxnportapi.MxNPort
  Defines 2 stop bits on serial communication
stopBits - Variable in class com.moxa.mxnportapi.MxNPort.IoctlMode
  Available constants: `STOP_BITS_1`, `STOP_BITS_1_5`, `STOP_BITS_2`.

B C D F G I L M O P R S V W X