
Product:    MXconfig Plug-in package
Version:    1.4
Date:       02/25/2023
Company:    Moxa Inc.

Support Platform:
-----------------
MXconfig 

Supported Product:
------------------------
- MGate Series MXconfig Plug-in package ver 1.8 Build 23022517
   Support MGate 5101-PBM-MN, MGate 5102-PBM-PN, MGate 5103, MGate 5105-MB-EIP,
           MGate 5108, MGate 5208, MGate 5109, MGate 5111, MGate 5114, 
           MGate 5118, MGate 5119, MGate 5217, MGate MB3170, MGate MB3170I, MGate MB3170 fiber series,
           MGate 5134, MGate 5135, MGate 5435, MGate 5121, MGate 5122, MGate 5123, MGate 5217-600-CN, MGate 5217I-1200-CN
           MGate MB3270, MGate MB3270I, MGate MB3180, MGate MB3280, MGate MB3480,
           MGate MB3660, MGate EIP3170, MGate EIP3170I, MGate EIP3270, MGate EIP3270I
           
 - MGate Series MXconfig Plug-in package ver 1.7 Build 20092415
   Support MGate 5101-PBM-MN, MGate 5102-PBM-PN, MGate 5103, MGate 5105-MB-EIP,
           MGate 5108, MGate 5208, MGate 5109, MGate 5111, MGate 5114, 
           MGate 5118, MGate 5217, MGate MB3170, MGate MB3170I, MGate MB3170 fiber series,
           MGate MB3270, MGate MB3270I, MGate MB3180, MGate MB3280, MGate MB3480,
           MGate MB3660, MGate EIP3170, MGate EIP3170I, MGate EIP3270, MGate EIP3270I

 - MGate Series MXconfig Plug-in package ver 1.6 Build 20073011
   Support MGate 5101-PBM-MN, MGate 5102-PBM-PN, MGate 5103, MGate 5105-MB-EIP,
           MGate 5108, MGate 5208, MGate 5109, MGate 5111, MGate 5114, 
           MGate 5118, MGate 5119, MGate MB3170, MGate MB3170I, MGate MB3170 fiber series,
           MGate MB3270, MGate MB3270I, MGate MB3180, MGate MB3280, MGate MB3480,
           MGate MB3660, MGate EIP3170, MGate EIP3170I, MGate EIP3270, MGate EIP3270I

 - NPort Series MXconfig Plug-in package ver1.3 Build 21032413
   Support NPort 5110 firmware ver3.8 or higher
           NPort 5130, 5150 firmware ver3.8 or higher
           NPort 5210, 5230, 5232, 5232I firmware ver2.10 or higher
           NPort 5410, 5430, 5430I, 5450, 5450I firmware ver3.13 or higher
           NPort 5610-8, 5610-8-48, 5610-16-48V firmware ver3.9 or higher
           NPort 5630-8, 5630-16 firmware ver3.9 or higher
           NPort 5650-8, 5650-16 firmware ver3.9 or higher
           NPort 5650-8-S-SC, 5650-8-M-SC, 5650-16-S-SC, 5650-16-M-SC 
           firmware ver3.9 or higher
           NPort 5610-8-DT, 5610-8-DT-J firmware ver2.6 or higher
           NPort 5650-8-DT, 5650I-8-DT, 5650-8-DT-J firmware ver2.6 or higher
           NPort 5610-8-DTL, 5650-8-DTL, 5650I-8-DTL firmware ver1.5 or higher
           NPort 5110A, 5130A, 5150A firmware ver1.5 or higher
           NPort 5210A, 5230A, 5250A firmware ver1.5 or higher
           NPort 5150AI-M12, 5250AI-M12, 5450AI-M12 firmware ver1.4 or higher.
           NPort IA5150, IA5150I, IA5250 firmware ver1.6 or higher
           NPort IA5150-M-SC, IA5150I-M-SC firmware ver1.6 or higher
           NPort IA5150-S-SC, IA5150I-S-SC firmware ver1.6 or higher
           NPort IA5150A, IA5150AI, IA5250A, IA5250AI firmware ver1.4 or higher
           NPort IA5450A, IA5450AI firmware ver1.6 or higher
   
   Support NPort 6000 Series: 
              6150, 6250, 6250-M-SC, 6250-S-SC, 6450, 6650-8, 6650-16 6610-8, 
              6610-16, 6610-32, 6650-32

 - NPort S8000/S9000 MXconfig Plug-in package ver1.2 Build 21102114
   Support NPort S8000 Series: S8455I-MM-SC, S8455I-SS-SC, S8458-4S-SC-T
   NPort S9000 Series:
           S9450I-WV, S9450I-MM-SC-WV, S9450I-MM-ST-WV, S9450I-SS-SC-WV,
           S9450I-SS-ST-WV, S9450I-HV, S9450I-MM-SC-HV, S9450I-MM-ST-HV,
           S9450I-SS-SC-HV, S9450I-SS-ST-HV, S9650I-8-2WV, S9650I-16-2WV,
           S9650I-8B-2WV, S9650I-16B-2WV, S9650I-8-2HV, S9650I-16-2HV, S9650I-8B-2HV,
           S9650I-16B-2HV, S9650I-16F-2HV, S9650I-16J-2HV

 - IO Series MXconfig Plug-in package ver1.2 Build 21041213
   Support ioLogik E1200 series: E1210(-T), E1211(-T), E1212(-T), E1213(-T),
                         E1214(-T), E1240(-T), E1241(-T), E1242(-T),
                         E1260(-T), E1262(-T)
   Support ioThinx 4510 series: ioThinx 4510(-T)

Release Note:
--------------
Ver 1.4 Build 23022517
1. Upgrade MGate Series MXconfig Plug-in package to ver 1.8 Build 23022517
   - New: Support new model MGate 5134, 5135, and 5435, MGate 5121, 5122, and 5123.

Ver 1.3 Build 21121711
1. Upgrade MGate Series MXconfig Plug-in package to ver 1.7.3 Build 21112313
   - New: Support new model MGate 5119, MGate 5217-600-CN and 5217I-1200-CN.
2. Upgrade NPort S8000/S9000 MXconfig Plug-in package to ver 1.2 Build 21102114.
   - New: Support NPort S9400/9600 firmware version 1.1.
   - New: Support security wizard, accessible IP and SNMP Configuration setting.

Ver 1.2 Build 21102211
1. Upgrade IO Series MXconfig Plug-in package to ver 1.2 Build 21071618.
   - New: Support syslog and https operation mode on ioThinx 4510.

Ver 1.1 Build 21032413
1. Upgrade MGate Series MXconfig Plug-in package to ver 1.7 Build 21032413.
   - New: Support new model MGate 5217I series.
   - Bugfix: MGate 5000 series should only support 16 indexes in accessible IP panel.
   - Bugfix: When enable account lockout, account shouldn't lockout after change password.
2. Upgrade IO Series MXconfig Plug-in package to ver 1.1 Build 21032413.
   - New: Support new model ioThinx 4510 series.
3. Upgrade NPort 5000/6000 Series MXconfig Plug-in package to ver 1.3 Build 21032413
   - New: Support NPort 6000 series firmware version 1.20.

Ver 1.1 Build 20120716
1. New: Support new model MGate 5217I-600 and 5217I-1200.

Ver 1.0 Build 20090815
1. Newly released. Package NPort 8000, NPort 5000/6000 and MGate series MXconfig plug-in in one installer.
2. Upgrade MGate Series MXconfig Plug-in package to ver 1.6 Build 20073011
   - Bugfix: In System Notification setting, Login Fail Message should not be delete by the length of the Web Login Message when over 240 characters.
   - Bugfix: In Accessible IP information overview page, MGate MB5000 series display the IP address in backwards.
   - Bugfix: In Security Wizard, MGate would reboot twice when change password.
3. Upgrade NPort Series MXconfig Plug-in package to ver1.2 Build 20090815
   - Bugfix: In System Notification setting, Login Fail Message should not be delete by the length of the Web Login Message when over 240 characters.