| ioPAC RTU Controllers C/C++ Sample Code Programming Guide

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- k
- l
- m
- n
- p
- r
- s
- t
- u
- v
- y

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - s -

- sec : libmoxa_rtu.h
- SERIAL_DATA_BITS_5 : libmoxa_rtu.h
- SERIAL_DATA_BITS_6 : libmoxa_rtu.h
- SERIAL_DATA_BITS_7 : libmoxa_rtu.h
- SERIAL_DATA_BITS_8 : libmoxa_rtu.h
- SERIAL_ERR_AMOUNT : libmoxa_rtu.h
- SERIAL_ERR_CLOSE : libmoxa_rtu.h
- SERIAL_ERR_CODE : libmoxa_rtu.h
- SERIAL_ERR_FD : libmoxa_rtu.h
- SERIAL_ERR_FLUSH : libmoxa_rtu.h
- SERIAL_ERR_HOT_PLUG : libmoxa_rtu.h
- SERIAL_ERR_IOCTL : libmoxa_rtu.h
- SERIAL_ERR_MODE : libmoxa_rtu.h
- SERIAL_ERR_NOT_SUPPORT_PRODUCT : libmoxa_rtu.h
- SERIAL_ERR_OK : libmoxa_rtu.h
- SERIAL_ERR_OPEN : libmoxa_rtu.h
- SERIAL_ERR_PARAMETER : libmoxa_rtu.h
- SERIAL_ERR_PORT : libmoxa_rtu.h
- SERIAL_ERR_READ : libmoxa_rtu.h
- SERIAL_ERR_SLOT : libmoxa_rtu.h
- SERIAL_ERR_SYSTEM_INFO : libmoxa_rtu.h
- SERIAL_ERR_ttyUSB : libmoxa_rtu.h
- SERIAL_ERR_WRITE : libmoxa_rtu.h
- SERIAL_MAX_OQUEUE_LENGTH : libmoxa_rtu.h
- serial_number : libmoxa_rtu.h
- SERIAL_PARITY_EVEN : libmoxa_rtu.h
- SERIAL_PARITY_NONE : libmoxa_rtu.h
- SERIAL_PARITY_ODD : libmoxa_rtu.h
- SERIAL_PORT : libmoxa_rtu.h
- SERIAL_STOP_BIT_1 : libmoxa_rtu.h
- SERIAL_STOP_BIT_2 : libmoxa_rtu.h
- SERVICE_AOPC_CONNCONTROL_PROFILE_TAG : ioPAC8500_aopc.c
- SERVICE_AOPC_STATUS_PROFILE_TAG : ioPAC8500_aopc.c
- SERVICE_AOPC_STATUS_TAG : ioPAC8500_aopc.c
- SERVICE_AOPC_TRIGGER_TAG : ioPAC8500_aopc.c
- SERVICE_MODBUSMASTER_STATUS_TAG : ioPAC8500_modbus_tcp_master_and_slave.c
- SERVICE_MODBUSSLAVE_STATUS_TAG : ioPAC8500_modbus_tcp_master_and_slave.c
- sig_handler() : fast_ai_stop.c
- SIZE_APN : libmoxa_rtu.h
- SIZE_HOSTNAME : libmoxa_rtu.h
- SIZE_IMEI : libmoxa_rtu.h
- SIZE_IP_ADDR : libmoxa_rtu.h
- SIZE_PASSWORD : libmoxa_rtu.h
- SIZE_PIN : libmoxa_rtu.h
- SIZE_USERNAME : libmoxa_rtu.h
- SLAVE_DEVICE_BUSY : libmoxa_rtu.h
- SLAVE_DEVICE_FAILURE : libmoxa_rtu.h
- slot : libmoxa_rtu.h
- SMS_ERR_AMOUNT : libmoxa_rtu.h
- SMS_ERR_CODE : libmoxa_rtu.h
- SMS_ERR_ERR : libmoxa_rtu.h
- SMS_ERR_ISP : libmoxa_rtu.h
- SMS_ERR_LENGTH : libmoxa_rtu.h
- SMS_ERR_MODEM : libmoxa_rtu.h
- SMS_ERR_NOT_SUPPORT_PRODUCT : libmoxa_rtu.h
- SMS_ERR_OK : libmoxa_rtu.h
- SMS_ERR_OPEN : libmoxa_rtu.h
- SMS_ERR_PDU : libmoxa_rtu.h
- SMS_ERR_PIN : libmoxa_rtu.h
- SMS_ERR_SYSTEM_INFO : libmoxa_rtu.h
- SOFTWARE_WATCHDOG_MAX_TIME : libmoxa_rtu.h
- SOFTWARE_WATCHDOG_MIN_TIME : libmoxa_rtu.h
- SRAM_END_ADDRESS : libmoxa_rtu.h
- SRAM_START_ADDRESS : libmoxa_rtu.h
- startHtml() : ai_cgi.c , ao_cgi.c , fast_ai_cgi.c , do_cgi.c , relay_cgi.c , di_cgi.c , tc_cgi.c , rtd_cgi.c
- startOneRow() : ao_cgi.c , do_cgi.c , rtd_cgi.c , tc_cgi.c , ai_cgi.c , fast_ai_cgi.c , di_cgi.c , relay_cgi.c
- startTable() : ai_cgi.c , di_cgi.c , do_cgi.c , ao_cgi.c , tc_cgi.c , relay_cgi.c , fast_ai_cgi.c , rtd_cgi.c
- STATUS_CODE : libmoxa_rtu.h
- STATUS_ERR_AMOUNT : libmoxa_rtu.h
- STATUS_FAIL : libmoxa_rtu.h
- STATUS_INIT : libmoxa_rtu.h
- STATUS_READY : libmoxa_rtu.h
- STATUS_RUNNING : libmoxa_rtu.h
- STATUS_SUCCESS : libmoxa_rtu.h
- stopHandler() : modbus_rtu_slave.c
- SW_FLOW_CONTROL : libmoxa_rtu.h
- SWITCH_DUMP_MODE : libmoxa_rtu.h
- SWITCH_VLAN_MODE : libmoxa_rtu.h