### Service/SNMP/snmp_agent_service/ioPAC8600_iec_snmp_agent_service/ioPAC8600_iec_snmp_agent_service_readme/ioPAC8600_iec_snmp_agent_service_readme.md

# ioPAC8600_iec_snmp_agent_service

## Detailed Description

### Background

ioPAC8600 snmp agent service IEC Sample Project

##### Copyright

Moxa Inc.

##### Date

07-27-2015

##### Author

TJ Tai

##### Version

V1.0

## Scenario

### Introduction

This is snmp agent service IEC sample project.

ioPAC8600_iec_snmp_agent_service scenario

## Operating Environment

### Hardware Environment

- CPU module:

    ioPAC8600-CPU10-RJ45-IEC-T

- Backplane module:

    ioPAC8600-BM009-T

- Slot 1:

    85M-1602-T

### Software Environment

- Programming Tool:

    ISaGRAF 6.3

- Configuration Tool:

    Moxa RTUxpress 1.4 Build 15040714

### Config Setting

Config file: ioPAC8600_iec_snmp_agent_service.rtu

## Step by Step

### Initialization

1. Open .rtu config file and setup your own setting (e.g. IP)
2. Import config file onto ioPAC via RTUxpress
3. Open IEC project via ISaGRAF
4. Build -> Build Solution on ISaGRAF
5. Import IEC porject onto ioPAC via ISaGRAF

### Step 1

If DI channel 0 on (connect to ground) and DI channel 15 on also, then IR tag: S0_IR_BOOL_Output0example will update to ON stuas.

### Step 2

Turn on snmp mib browser (e.g. IReasoning Mib browser) and load the mib file which can be found under `/etc/snmp` on ioPAC to monitor this IR tag in tagtable

## Reference

- ISaGRAF Function Block Help:

  > please press F1 button on the function block which need more description in the ISaGRAF

- Moxa ioPAC ISaGRAF Reference Manuals:

  > Please press Help -> Moxa ioPAC ISaGRAF Reference Manuals in the Moxa RTUxpress utility