Readme for TCPClient2 example program

1. Overview
The example programs explain you how to write a simple TCP Client program
to communicate with PC. The examples uses both standard BSD Sockets and
simplified Sockets.

2. The Hardware connection is following:
Terminal---(RS232)[UC/DA serials]--- ~~LAN~~ ---PC Host Example

3. Files

Directory: ..\NESDK\Example\TCPClient2

tcpc.c
-TCP Client program for UC/DA serials using standard BSD Sockets APIs

TCPServer2_PC\VC\Release\tcpserver.exe
- TCP Server program running in Windows98/2000/XP.
- Visual Basic version is also available in ..\VB

4. How to use the example program
 4.1 Run TCP server program from a networked PC and ready to get data from the UC/DA serials or send data to the UC/DA serials.
 4.2 Run serial terminal program from a networked PC and ready to get serial data from the UC/DA serials or send serial data to the UC/DA serials.
 4.3 Download tcpc2-release or tcpc2-debug to the UC/DA serials. Then run the application. 
