EPM-3032, EPM-3337, EPM-3438,EPM-3112 are the expension module for V2422/V2426 Embedded Computers.

Copyright (C) 2004-2011 Moxa Systems Co., Ltd.

*************************************************************************
V2422, V2426 ..... 

features low-heat yet high-performance CPU with networking 
and serial design within a rugged enclosure. These features make 
this embedded computer suitable for front end data acquistion in 
diverse control systems.

Download useful information from the download center at 
http://www.moxa.com/
*************************************************************************

Files & Directories:

 * README.txt -- this file.

 * EPM-3032  -- serial port expension module

    driver   -- EPM-3032 driverpackage

    sdk      -- EPM-3032 library

    examples -- EPM-3032 example code

 * EPM-3337 -- 802.11 b/g/n and GPS expension module.

    driver  -- EPM-3337 driver package 

 * EPM-3438 -- Digital I/O / Counter module.

    driver  -- EPM-3438 driver package 

    sdk     -- EPM-3438 library

    examples -- EPM-3438 example code	

 * EPM-3112 -- CANBUS module.

    driver  -- EPM-3112 driver package 

    sdk     -- EPM-3112 library

    examples -- EPM-3112 example code	


 * EPM-DK02 -- MiniPCIe expansion module.

    driver  -- EPM-DK02 driver  

    examples -- EPM-DK02 example code

*************************************************************************
Driver Installation for EPM-DK02
(Note: You have to install the WatchDog driver before using this function.)
*************************************************************************
 Start-> Control Panel -> Double click "Add Hardware" and follow below instructions.
1. Is the hardware connected? -> Tick "Yes".
2. Select "Add a new hardware device" -> Click "Next".
3. Install hardware that I manually select from a list [Advanced] -> Next
4. Select "Device Drivers" -> Next
5. Select the device driver you want to install for the hardware -> Click "Have Disk..."
6. Install From Disk -> Click "Browse..." to find the folder of "driver" in this package. -> OK
7. Select the device driver you want to install for the hardware -> Click "Next".
8. Finish.

