
Product:	NPort Windows Driver Manager (XP Embedded)
Version:	1.14 Build 11042017
Date:		04/20/2011
Company:	Moxa Inc.


Support Platform:
-----------------
Windows XP Embedded

Supported Moxa Product:
------------------------
CN2500 Series: CN2510-8, CN2510-16, CN2510-8-48V, CN2510-16-48V
CN2600 Series: CN2610-8, CN2610-16, CN2650-8, CN2650-16, CN2650I-8, CN2650I-16,
               CN2610-8-2AC, CN2610-16-2AC, CN2650-8-2AC, CN2650-16-2AC,
               CN2650I-8-2AC, CN2650I-16-2AC
NPort: DE-211, DE-311, DE-311M, DE-301, DE-302, DE-304, DE-334
NPort 5100 Series: 5110, 5130, 5150, 5110A, 5130A, 5150A
NPort 5200 Series: 5210, 5230, 5232, 5232I, 5210A, 5230A, 5250A
NPort 5400 Series: 5410, 5410 V3, 5430, 5430 V3, 5430I, 5430I V3, 5450, 5450I
NPort 5600 Rackmount Serise: 5610-8, 5610-16, 5610-8-48V, 5610-16-48V, 
                             5630-8, 5630-16, 5650-8, 5650-16,
                             5650-8-M-SC, 5650-16-M-SC, 5650-8-S-SC,
                             5650-16-S-SC
NPort 5600 Desktop Series: 5610-8-DT, 5610-8-DT-J, 5650-8-DT, 5650I-8-DT, 
                           5650-8-DT-J
NPort 5600 Desktop Lite Series: 5610-8-DTL, 5650-8-DTL, 5650I-8-DTL                           
NPort IA Series: IA-5150, IA-5150I, IA-5150-S-SC, IA-5150I-S-SC, IA-5150-M-SC,
                 IA-5150I-M-SC, IA-5250, IA-5250I, IA5450A, IA5450AI,
                 IA5150A, IA5150AI, IA5250A, IA5250AI
NPort 6000 Series: 6150, 6250, 6250-M-SC, 6250-S-SC, 6450, 6650-8, 6650-16
                   6610-8, 6610-16, 6610-32, 6650-32
NPort S8000 Series: NPort S8455I-MM-SC, NPort S8455I-SS-SC, NPort S8455I,
                    NPort S8458-4S-SC-T
NPort Wireless Series: W2004, W2150, W2250, W2150 Plus, W2250 Plus, WE-2100T
NE Series: 4100T, 4100T-CMD, 4110A, 4110A-CMD, 4110S, 4110S-CMD,
           4120A, 4120A-CMD, 4120S, 4120S-CMD
MiiNePort Series: E1, E1-P, E1-H, E2, E2-H

Release Note:
--------------
Ver1.14 Build 11042017 (04/20/2011)
1. New: Support NPort S8458-4S-SC-T.
2. New: Support NPort 5600 DTL series.
3. New: NPort driver will agree to open COM port on the system even if the port 
        is blocked or the Ethernet connection is disabled.
4. Bugfix: DE-2XX and DE-3XX series cannot be searched if the number of devices
           is more than four.
5. Bugfix: NPort device cannot be found by utility via wireless network adapter
           under Windows Vista/7.
6. Bugfix: Driver causes system BSOD by writing to an invalid memory location 
           under Windows 2008 64bit.
7. Bugfix: The application will not work properly when login with standard user
           in Windows Vista/7 environment. This version will prompt user change
           to account with administration rights.

-END-
