                          NPort series
             Driver Component for Windows XP Embedded
                           2011/04/20
                   Copyright (C) 2011 Moxa Inc.

1. Import the driver component
(1) Copy all the files to a directory, e.g. "C:\NPort\".
(2) Open Component Database Manager under Microsoft Windows Embedded Studio.
(3) Click on the "Repository" and then "Repository Roots..." buttons.
    Type in the complete path of the repositories directory,
    for example "C:\NPort\". Click on the "Add" button and answer "Yes". 
(4) Click on the "Database", "Import...", and then "..." buttons.
    Navigate to directory "C:\NPort\" and then choose
    the .SLD file. Next, pull down "Repository root" drop-down
    and select "C:\NPort\". Click on the "Import" and
    then "Close" buttons to close the dialog.
(5) Close the "Component Database Manager".
