Version Number: 2.0 
Product Line:   UPort 1200/1400/1600 Series Driver for Linux
Platform:       Linux kernel 2.6.x (x86/x64)
Company:        Moxa Inc.
Date:           2019/05/02

Support Product:
===============
UPort 1250, 1250I
UPort 1410, 1450, 1450I 
UPort 1610-8, 1650-8 
UPort 1610-16, 1650-16 

Tested Linux: 
=============
Kernel 2.6.39
Kernel 2.6.36
Kernel 2.6.30.1
Kernel 2.6.30
Kernel 2.6.28
Kernel 2.6.26
Fedora 8 (2.6.23)
Fedora 7 (2.6.22)
Fedora Core 6 (2.6.18)
Fedora Core 5 (2.6.15)
Fedora Core 4 (2.6.11)
Fedora Core 3 (2.6.9)
Fedora Core 2 (2.6.5)

SuSE 10.3 (2.6.22)
SuSE 10.1 (2.6.16)
SuSE 9.3 (2.6.11)

Ubuntu 8.04 (2.6.24)
Ubuntu 7.10 (2.6.22)

Red Hat Enterprise Linux Release 4 (2.6.9)

Release Note:
==============
Ver2.0
1. Improve: Support to disable FIFO by setserial utility.
2. Bugfix: Fix the issue that modem status is not correct after ports are
           opened.
3. Change: Divided an independent driver version 2.0 to support Linux kernel
           2.6.x.

Ver1.2
1. New: Support kernel version up to 3.4.4
2. Bugfix: Fix bug of compiling fail under gcc version 3.3.3. 
3. Bugfix: Fixed system memory leak when application keeps doing open/close 
           operations for a long time execution.
4. Bugfix: Fixed application hang up when open/close frequencytly.

Ver1.1
1. New: Support auto installation.

Ver1.0
1. New: Official released.

-End-
