- Main
- Tutorials
- Library
- Samples

Modules | Functions
IoThinx_IO
Library

## Modules
| IOTHINX_ERR
| IOTHINX_BUS_STATUS

## Functions
IOTHINX_ERR | ioThinx_IO_Client_Init (void)
IOTHINX_ERR | ioThinx_IO_GetBusStatus (uint8_t *p_status)
IOTHINX_ERR | ioThinx_IO_Config_Reload (void)

## Detailed Description

## Function Documentation

IOTHINX_ERR ioThinx_IO_Client_Init | ( | void |  | ) |

Returns
  IOTHINX_ERR_OK if everything is ok. Otherwise, refer to the IOTHINX_ERR.

Note
  This function MUST be called before using ioThinx library.

IOTHINX_ERR ioThinx_IO_GetBusStatus | ( | uint8_t * | p_status | ) |

Parameters

  [out] | p_status | A pointer that stores I/O bus status.

Returns
  IOTHINX_ERR_OK if everything is ok. Otherwise, refer to the IOTHINX_ERR.

IOTHINX_ERR ioThinx_IO_Config_Reload | ( | void |  | ) |

Returns
  IOTHINX_ERR_OK if everything is ok. Otherwise, refer to the IOTHINX_ERR.

Note
  This function MUST be called after using ioThinx config APIs. Config will not be loaded to the I/O modules until this function called.