B C D F G I L M O P R S V W X

## G

getBaud() - Method in interface com.moxa.mxnportapi.MxNPort
  Get the serial port baud rate setting.
getFlowCtrl() - Method in interface com.moxa.mxnportapi.MxNPort
  Get the serial port's hardware and software flow control settings.
getIoctlMode() - Method in interface com.moxa.mxnportapi.MxNPort
  Gets the serial port's mode settings, such as data bits, parity, and stop bits.
getLineStatus() - Method in interface com.moxa.mxnportapi.MxNPort
  Checks if errors occurred when receiving data, such as overrun error, parity error, framing error and break_error.
getModemStatus() - Method in interface com.moxa.mxnportapi.MxNPort
  Gets the line status, such as CTS, DSR, DCD, or RI.
getNPortInfoList() - Static method in class com.moxa.mxnportapi.MxNPortService
  Builds and returns a new List<`MxNPort`> from the connected NPort in the same subnet, or returns `null` if a NPort is not available in system.
getNPortIPAddress(int) - Method in interface com.moxa.mxnportapi.MxNPort
  Returns the IP address of a NPort devices.
getNPortMACAddress(int) - Method in interface com.moxa.mxnportapi.MxNPort
  Returns the MAC address of a NPort devices.
getNPortMaximumPort() - Method in interface com.moxa.mxnportapi.MxNPort
  Returns the total serial port number of a NPort device.
getNPortModelName() - Method in interface com.moxa.mxnportapi.MxNPort
  Returns the model name of a NPort device.
getNPortPortIndex() - Method in interface com.moxa.mxnportapi.MxNPort
  Returns the using serial port number of a NPort device.
getOQueue() - Method in interface com.moxa.mxnportapi.MxNPort
  Gets the length (in bytes) remaining in the NPort's output buffer.
getString() - Method in enum com.moxa.mxnportapi.MxException.ErrorCode
  Get the description of this error.
getString() - Static method in class com.moxa.mxnportapi.Version
  Gets a version string.

B C D F G I L M O P R S V W X